From f8bef3619bb219ed27dfe11cd20547e5b709650a Mon Sep 17 00:00:00 2001
From: Gerd Hoffmann <kraxel@redhat.com>
Date: Mon, 19 Sep 2016 10:43:22 +0200
Subject: [PATCH] ARM: dts: bcm283x: add pinctrl group to &sdhci, drop pins
 from &gpio

Signed-off-by: Gerd Hoffmann <kraxel@redhat.com>
Signed-off-by: Eric Anholt <eric@anholt.net>
Acked-by: Stefan Wahren <stefan.wahren@i2se.com>
---
 arch/arm/boot/dts/bcm2835-rpi.dtsi | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm2835-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2835-rpi.dtsi
@@ -44,7 +44,7 @@
 	};
 
 	alt3: alt3 {
-		brcm,pins = <48 49 50 51 52 53>;
+		brcm,pins = <>;
 		brcm,function = <BCM2835_FSEL_ALT3>;
 	};
 };
@@ -68,6 +68,8 @@
 };
 
 &sdhci {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emmc_gpio48>;
 	status = "okay";
 	bus-width = <4>;
 };
