From 1647cccc871bf43876c3df9852869680880d054c Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Wed, 25 Mar 2015 13:52:02 +0100
Subject: [PATCH 1/2] MIPS: BCM63XX: provide a gpio lookup for the pcmcia
 ready gpio

To prepare for a time when gpiobases don't need to be fixed anymore.

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/dev-pcmcia.c |   13 +++++++++++++
 1 file changed, 13 insertions(+)

--- a/arch/mips/bcm63xx/dev-pcmcia.c
+++ b/arch/mips/bcm63xx/dev-pcmcia.c
@@ -10,6 +10,7 @@
 #include <linux/kernel.h>
 #include <asm/bootinfo.h>
 #include <linux/platform_device.h>
+#include <linux/gpio/machine.h>
 #include <bcm63xx_cs.h>
 #include <bcm63xx_cpu.h>
 #include <bcm63xx_dev_pcmcia.h>
@@ -101,6 +102,14 @@ static const struct {
 	},
 };
 
+static struct gpiod_lookup_table pcmcia_gpios_table = {
+	.dev_id = "bcm63xx_pcmcia.0",
+	.table = {
+		GPIO_LOOKUP("bcm63xx-gpio.0", 0, "ready", GPIO_ACTIVE_HIGH),
+		{ },
+	},
+};
+
 int __init bcm63xx_pcmcia_register(void)
 {
 	int ret, i;
@@ -112,16 +121,20 @@ int __init bcm63xx_pcmcia_register(void)
 	switch (bcm63xx_get_cpu_id()) {
 	case BCM6348_CPU_ID:
 		pd.ready_gpio = 22;
+		pcmcia_gpios_table.table[0].chip_hwnum = 22;
 		break;
 
 	case BCM6358_CPU_ID:
 		pd.ready_gpio = 18;
+		pcmcia_gpios_table.table[0].chip_hwnum = 18;
 		break;
 
 	default:
 		return -ENODEV;
 	}
 
+	gpiod_add_lookup_table(&pcmcia_gpios_table);
+
 	pcmcia_resources[0].start = bcm63xx_regset_address(RSET_PCMCIA);
 	pcmcia_resources[0].end = pcmcia_resources[0].start +
 		RSET_PCMCIA_SIZE - 1;
