From dbda7dacb79a377e8ed9d38ce0e4a58b70aa9060 Mon Sep 17 00:00:00 2001
From: Arend Van Spriel <arend.vanspriel@broadcom.com>
Date: Tue, 19 Dec 2017 13:47:08 +0100
Subject: [PATCH] brcmfmac: Rename buscore to core for consistency

Avoid confusion with unrelated _buscore labels.

Signed-off-by: Ian Molton <ian@mnementh.co.uk>
Acked-by: Arend van Spriel <arend.vanspriel@broadcom.com>
[arend: only do the rename]
Signed-off-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -2485,12 +2485,12 @@ static inline void brcmf_sdio_clrintr(st
 
 static int brcmf_sdio_intr_rstatus(struct brcmf_sdio *bus)
 {
-	struct brcmf_core *buscore = bus->sdio_core;
+	struct brcmf_core *core = bus->sdio_core;
 	u32 addr;
 	unsigned long val;
 	int ret;
 
-	addr = buscore->base + SD_REG(intstatus);
+	addr = core->base + SD_REG(intstatus);
 
 	val = brcmf_sdiod_readl(bus->sdiodev, addr, &ret);
 	bus->sdcnt.f1regdata++;
