From: Felix Fietkau <nbd@nbd.name>
Subject: block2mtd

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---
 drivers/mtd/devices/block2mtd.c | 30 ++++++++++++++++++++----------
 1 file changed, 20 insertions(+), 10 deletions(-)

--- a/drivers/mtd/devices/block2mtd.c
+++ b/drivers/mtd/devices/block2mtd.c
@@ -26,6 +26,7 @@
 #include <linux/list.h>
 #include <linux/init.h>
 #include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
 #include <linux/mutex.h>
 #include <linux/mount.h>
 #include <linux/slab.h>
@@ -219,7 +220,7 @@ static void block2mtd_free_device(struct
 
 
 static struct block2mtd_dev *add_device(char *devname, int erase_size,
-		int timeout)
+		const char *mtdname, int timeout)
 {
 #ifndef MODULE
 	int i;
@@ -227,6 +228,7 @@ static struct block2mtd_dev *add_device(
 	const fmode_t mode = FMODE_READ | FMODE_WRITE | FMODE_EXCL;
 	struct block_device *bdev = ERR_PTR(-ENODEV);
 	struct block2mtd_dev *dev;
+	struct mtd_partition *part;
 	char *name;
 
 	if (!devname)
@@ -283,13 +285,16 @@ static struct block2mtd_dev *add_device(
 
 	/* Setup the MTD structure */
 	/* make the name contain the block device in */
-	name = kasprintf(GFP_KERNEL, "block2mtd: %s", devname);
+	if (!mtdname)
+		mtdname = devname;
+	name = kmalloc(strlen(mtdname) + 1, GFP_KERNEL);
 	if (!name)
 		goto err_destroy_mutex;
 
+	strcpy(name, mtdname);
 	dev->mtd.name = name;
 
-	dev->mtd.size = dev->blkdev->bd_inode->i_size & PAGE_MASK;
+	dev->mtd.size = dev->blkdev->bd_inode->i_size & PAGE_MASK & ~(erase_size - 1);
 	dev->mtd.erasesize = erase_size;
 	dev->mtd.writesize = 1;
 	dev->mtd.writebufsize = PAGE_SIZE;
@@ -302,7 +307,11 @@ static struct block2mtd_dev *add_device(
 	dev->mtd.priv = dev;
 	dev->mtd.owner = THIS_MODULE;
 
-	if (mtd_device_register(&dev->mtd, NULL, 0)) {
+	part = kzalloc(sizeof(struct mtd_partition), GFP_KERNEL);
+	part->name = name;
+	part->offset = 0;
+	part->size = dev->mtd.size;
+	if (mtd_device_register(&dev->mtd, part, 1)) {
 		/* Device didn't get added, so free the entry */
 		goto err_destroy_mutex;
 	}
@@ -310,8 +319,7 @@ static struct block2mtd_dev *add_device(
 	list_add(&dev->list, &blkmtd_device_list);
 	pr_info("mtd%d: [%s] erase_size = %dKiB [%d]\n",
 		dev->mtd.index,
-		dev->mtd.name + strlen("block2mtd: "),
-		dev->mtd.erasesize >> 10, dev->mtd.erasesize);
+		mtdname, dev->mtd.erasesize >> 10, dev->mtd.erasesize);
 	return dev;
 
 err_destroy_mutex:
@@ -384,7 +392,7 @@ static int block2mtd_setup2(const char *
 	/* 80 for device, 12 for erase size, 80 for name, 8 for timeout */
 	char buf[80 + 12 + 80 + 8];
 	char *str = buf;
-	char *token[2];
+	char *token[3];
 	char *name;
 	size_t erase_size = PAGE_SIZE;
 	unsigned long timeout = MTD_DEFAULT_TIMEOUT;
@@ -398,7 +406,7 @@ static int block2mtd_setup2(const char *
 	strcpy(str, val);
 	kill_final_newline(str);
 
-	for (i = 0; i < 2; i++)
+	for (i = 0; i < 3; i++)
 		token[i] = strsep(&str, ",");
 
 	if (str) {
@@ -424,8 +432,10 @@ static int block2mtd_setup2(const char *
 			return 0;
 		}
 	}
+	if (token[2] && (strlen(token[2]) + 1 > 80))
+		pr_err("mtd device name too long\n");
 
-	add_device(name, erase_size, timeout);
+	add_device(name, erase_size, token[2], timeout);
 
 	return 0;
 }
@@ -459,7 +469,7 @@ static int block2mtd_setup(const char *v
 
 
 module_param_call(block2mtd, block2mtd_setup, NULL, NULL, 0200);
-MODULE_PARM_DESC(block2mtd, "Device to use. \"block2mtd=<dev>[,<erasesize>]\"");
+MODULE_PARM_DESC(block2mtd, "Device to use. \"block2mtd=<dev>[,<erasesize>[,<name>]]\"");
 
 static int __init block2mtd_init(void)
 {
