From 78d5fab8e345b1273ec8c22d06f1a1d27670b518 Mon Sep 17 00:00:00 2001
From: Philipp Tomsich <philipp.tomsich@theobroma-systems.com>
Date: Tue, 16 Jun 2015 10:59:38 +0200
Subject: ARM: sunxi: Make CONS_INDEX configurable


--- a/arch/arm/mach-sunxi/Kconfig
+++ b/arch/arm/mach-sunxi/Kconfig
@@ -416,6 +416,14 @@ config SYS_BOARD
 config SYS_SOC
 	default "sunxi"
 
+config CONS_INDEX
+        int "UART used for console"
+        range 1 5
+        default 1
+        ---help---
+        Defines the UART port used for serial output. It starts at 1 so UART0 is 1,
+        UART1 is 2 and so on.
+
 config UART0_PORT_F
 	bool "UART0 on MicroSD breakout board"
 	default n
