From 4a849cef15885cf5dd901fafe45d3fa51b2b2a09 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 9 Feb 2017 14:33:30 +0000
Subject: [PATCH] irq-bcm2836: Avoid "Invalid trigger warning"

Initialise the level for each IRQ to avoid a warning from the
arm arch timer code.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/irqchip/irq-bcm2836.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/irqchip/irq-bcm2836.c
+++ b/drivers/irqchip/irq-bcm2836.c
@@ -178,7 +178,7 @@ static void bcm2836_arm_irqchip_register
 
 	irq_set_percpu_devid(irq);
 	irq_set_chip_and_handler(irq, chip, handle_percpu_devid_irq);
-	irq_set_status_flags(irq, IRQ_NOAUTOEN);
+	irq_set_status_flags(irq, IRQ_NOAUTOEN | IRQ_TYPE_LEVEL_LOW);
 }
 
 static void
