#!/bin/sh
#
# Copyright (c) 2015 The Linux Foundation. All rights reserved.
# Copyright (c) 2011-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

board_config_update

board=$(board_name)

case "$board" in
compex,wpq864 |\
netgear,d7800 |\
netgear,r7500 |\
netgear,r7500v2 |\
qcom,ipq8064-ap148 |\
tplink,vr2600v)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "6@eth1" "5:wan" "0@eth0"
	;;
linksys,ea8500)
	hw_mac_addr=$(mtd_get_mac_ascii devinfo hw_mac_addr)
	ucidef_add_switch "switch0" \
		"0@eth0" "1:lan" "2:lan" "3:lan" "4:lan" "5:wan"
	ucidef_set_interface_macaddr "lan" "$hw_mac_addr"
	ucidef_set_interface_macaddr "wan" "$hw_mac_addr"
	;;
nec,wg2600hp)
	ucidef_add_switch "switch0" \
		"2:lan" "3:lan" "4:lan" "5:lan" "6@eth1" "1:wan" "0@eth0"
	;;
netgear,r7800 |\
tplink,c2600)
	ucidef_add_switch "switch0" \
		"1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "6@eth1" "5:wan" "0@eth0"
	;;
qcom,ipq8064-db149)
	ucidef_set_interface_lan "eth1 eth2 eth3"
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "6u@eth1" "5:wan" "0u@eth0"
	;;
zyxel,nbg6817)
	hw_mac_addr=$(mtd_get_mac_ascii 0:APPSBLENV ethaddr)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "6@eth1" "5:wan" "0@eth0"
	ucidef_set_interface_macaddr "lan" "$(macaddr_add $hw_mac_addr 2)"
	ucidef_set_interface_macaddr "wan" "$(macaddr_add $hw_mac_addr 3)"
	;;
*)
	echo "Unsupported hardware. Network interfaces not intialized"
	;;
esac

board_config_flush

exit 0
