From 317560a92ebfdac14df54b6a242dd8f5ecc1fd58 Mon Sep 17 00:00:00 2001
From: Robert Tiemann <rtie@gmx.de>
Date: Mon, 20 Jul 2015 11:01:25 +0200
Subject: [PATCH] BCM2835_DT: Fix I2S register map

---
 Documentation/devicetree/bindings/dma/brcm,bcm2835-dma.txt   | 4 ++--
 Documentation/devicetree/bindings/sound/brcm,bcm2835-i2s.txt | 4 ++--
 2 files changed, 4 insertions(+), 4 deletions(-)

--- a/Documentation/devicetree/bindings/dma/brcm,bcm2835-dma.txt
+++ b/Documentation/devicetree/bindings/dma/brcm,bcm2835-dma.txt
@@ -74,8 +74,8 @@ Example:
 
 bcm2835_i2s: i2s@7e203000 {
 	compatible = "brcm,bcm2835-i2s";
-	reg = <	0x7e203000 0x20>,
-	      < 0x7e101098 0x02>;
+	reg = <	0x7e203000 0x24>,
+	      < 0x7e101098 0x08>;
 
 	dmas = <&dma 2>,
 	       <&dma 3>;
--- a/Documentation/devicetree/bindings/sound/brcm,bcm2835-i2s.txt
+++ b/Documentation/devicetree/bindings/sound/brcm,bcm2835-i2s.txt
@@ -16,8 +16,8 @@ Example:
 
 bcm2835_i2s: i2s@7e203000 {
 	compatible = "brcm,bcm2835-i2s";
-	reg = <0x7e203000 0x20>,
-	      <0x7e101098 0x02>;
+	reg = <0x7e203000 0x24>,
+	      <0x7e101098 0x08>;
 
 	dmas = <&dma 2>,
 	       <&dma 3>;
