From 022a400f90ceeb26405edd5e077d56e2f38c8123 Mon Sep 17 00:00:00 2001
From: Sean Nyekjaer <sean.nyekjaer@prevas.dk>
Date: Wed, 5 Oct 2016 10:59:49 +0200
Subject: [PATCH] mtd: spi-nor: add support for s25fl208k

Signed-off-by: Sean Nyekjaer <sean.nyekjaer@prevas.dk>
Reviewed-by: Jagan Teki <jagan@openedev.com>
Acked-by: Marek Vasut <marex@denx.de>
Signed-off-by: Cyrille Pitchen <cyrille.pitchen@atmel.com>
---
 drivers/mtd/spi-nor/spi-nor.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -922,6 +922,7 @@ static const struct flash_info spi_nor_i
 	{ "s25fl132k",  INFO(0x014016,      0,  64 * 1024,  64, SECT_4K) },
 	{ "s25fl164k",  INFO(0x014017,      0,  64 * 1024, 128, SECT_4K) },
 	{ "s25fl204k",  INFO(0x014013,      0,  64 * 1024,   8, SECT_4K | SPI_NOR_DUAL_READ) },
+	{ "s25fl208k",  INFO(0x014014,      0,  64 * 1024,  16, SECT_4K | SPI_NOR_DUAL_READ) },
 
 	/* SST -- large erase sizes are "overlays", "sectors" are 4K */
 	{ "sst25vf040b", INFO(0xbf258d, 0, 64 * 1024,  8, SECT_4K | SST_WRITE) },
