From 072b6e3692532b6281bf781ded1c7a986ac17471 Mon Sep 17 00:00:00 2001
From: Corentin Labbe <clabbe.montjoie@gmail.com>
Date: Thu, 6 Jul 2017 10:53:34 +0200
Subject: ARM: dts: sunxi: h3/h5: Correct emac register size

The datasheet said that emac register size is 0x10000 not 0x104

Signed-off-by: Corentin Labbe <clabbe.montjoie@gmail.com>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
[wens@csie.org: Fixed commit subject prefix]
Signed-off-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm/boot/dts/sunxi-h3-h5.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/sun8i-h3.dtsi
+++ b/arch/arm/boot/dts/sun8i-h3.dtsi
@@ -442,7 +442,7 @@
 		emac: ethernet@1c30000 {
 			compatible = "allwinner,sun8i-h3-emac";
 			syscon = <&syscon>;
-			reg = <0x01c30000 0x104>;
+			reg = <0x01c30000 0x10000>;
 			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
 			interrupt-names = "macirq";
 			resets = <&ccu RST_BUS_EMAC>;
