/dts-v1/;

#include "rt3050.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "netgear,wnce2001", "ralink,rt3052-soc";
	model = "Netgear WNCE2001";

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	gpio-leds {
		compatible = "gpio-leds";

		power-green {
			label = "wnce2001:green:power";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		power-red {
			label = "wnce2001:red:power";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		wlan-green {
			label = "wnce2001:green:wlan";
			gpios = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		};

		wlan-red {
			label = "wnce2001:red:wlan";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		rt {
			label = "rt";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		ap {
			label = "ap";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x30000>;
			read-only;
		};

		factory: partition@30000 {
			label = "factory";
			reg = <0x30000 0x10000>;
			read-only;
		};

		partition@40000 {
			label = "config";
			reg = <0x40000 0x20000>;
			read-only;
		};

		partition@60000 {
			label = "language";
			reg = <0x60000 0x30000>;
			read-only;
		};

		partition@90000 {
			label = "pot";
			reg = <0x90000 0x10000>;
			read-only;
		};

		partition@a0000 {
			label = "checksum";
			reg = <0xa0000 0x10000>;
		};

		partition@b0000 {
			label = "firmware";
			reg = <0xb0000 0x350000>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "jtag", "rgmii", "mdio", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
