--- a/arch/arm/boot/dts/qcom-ipq4019-ap.dk01.1-c1.dts
+++ b/arch/arm/boot/dts/qcom-ipq4019-ap.dk01.1-c1.dts
@@ -18,6 +18,7 @@
 
 / {
 	model = "Qualcomm Technologies, Inc. IPQ40xx/AP-DK01.1-C1";
+	compatible = "qcom,ap-dk01.1-c1", "qcom,ap-dk01.2-c1", "qcom,ipq4019";
 
 	memory {
 		device_type = "memory";
