/dts-v1/;

#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv8539pw22", "lantiq,xway", "lantiq,danube";
	model = "Speedport W 504V Typ A";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;

		led-dsl = &dsl_green;
		led-internet = &online_green;
		led-wifi = &wireless_green;
	};

	memory@0 {
		reg = <0x0 0x4000000>;
	};

	sram@1F000000 {
		vmmc@107000 {
			status = "okay";
			gpios = <&gpio 31 GPIO_ACTIVE_HIGH>;
		};
	};

	fpi@10000000 {
		localbus@0 {
			nor-boot@0 {
				compatible = "lantiq,nor";
				bank-width = <2>;
				reg = <0 0x0 0x800000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partitions {
					compatible = "fixed-partitions";
					#address-cells = <1>;
					#size-cells = <1>;

					partition@0 {
						label = "uboot";
						reg = <0x00000 0x30000>;	/* 192 KiB */
						read-only;
					};

					partition@30000 {
						label = "uboot";
						reg = <0x30000 0x10000>;	/* 64 KiB */
						read-only;
					};

					partition@40000 {
						label = "firmware";
						reg = <0x40000 0x7B0000>;       /* 7872 KiB */
					};

					art: partition@7F0000 {
						label = "art";
						reg = <0x7F0000 0x10000>;       /* 64 KiB*/
						read-only;
					};
				};
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			state_default: pinmux {
				pci_in {
					lantiq,groups = "req1";
					lantiq,function = "pci";
					lantiq,open-drain = <1>;
					lantiq,pull = <2>;
					lantiq,output = <0>;
				};
				pci_out {
					lantiq,groups = "gnt1";
					lantiq,function = "pci";
					lantiq,output = <1>;
				};
				pci_rst {
					lantiq,pins = "io21";
					lantiq,pull = <2>;
					lantiq,output = <1>;
				};
				relay {
					lantiq,pins = "io31";
					lantiq,output = <1>;
				};
			};
		};

		etop@E180000 {
			phy-mode = "mii";
			mtd-mac-address = <&art 0x16>;
		};

		ifxhcd@E101000 {
			status = "okay";
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
			lantiq,portmask = <0x3>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		wlan {
			label = "wlan";
			gpios = <&gpio 29 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		/* key DECT is missing */
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_green: power-green {
			label = "arv8539pw22:green:power";
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power-red {
			label = "arv8539pw22:red:power";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		dsl_green: dsl-green {
			label = "arv8539pw22:green:dsl";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};

		online_green: online-green {
			label = "arv8539pw22:green:online";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		wireless_green: wireless-green {
			label = "arv8539pw22:green:wlan";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		/*
			telefonie green is missing
		*/
	};
};

&pci0 {
	status = "okay";
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;

	wifi@168c,0029 {
		compatible = "pci168c,0029";
		reg = <0x7000 0 0 0 0>;
		qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:00:0e.0.bin */
		mtd-mac-address = <&art 0x16>;
		mtd-mac-address-increment = <1>;
	};
};
