From 8f444887e23b9f0ea31aaae74fbc18171714d8d2 Mon Sep 17 00:00:00 2001
From: Chunfeng Yun <chunfeng.yun@mediatek.com>
Date: Fri, 13 Oct 2017 17:10:43 +0800
Subject: [PATCH 109/224] usb: mtu3: add support for usb3.1 IP

Support SuperSpeedPlus for usb3.1 device IP

Signed-off-by: Chunfeng Yun <chunfeng.yun@mediatek.com>
Signed-off-by: Felipe Balbi <felipe.balbi@linux.intel.com>
---
 drivers/usb/mtu3/mtu3.h            |  1 +
 drivers/usb/mtu3/mtu3_core.c       | 14 +++++++++++---
 drivers/usb/mtu3/mtu3_gadget.c     |  3 ++-
 drivers/usb/mtu3/mtu3_gadget_ep0.c | 16 ++++++++--------
 drivers/usb/mtu3/mtu3_hw_regs.h    |  1 +
 5 files changed, 23 insertions(+), 12 deletions(-)

--- a/drivers/usb/mtu3/mtu3.h
+++ b/drivers/usb/mtu3/mtu3.h
@@ -94,6 +94,7 @@ enum mtu3_speed {
 	MTU3_SPEED_FULL = 1,
 	MTU3_SPEED_HIGH = 3,
 	MTU3_SPEED_SUPER = 4,
+	MTU3_SPEED_SUPER_PLUS = 5,
 };
 
 /**
--- a/drivers/usb/mtu3/mtu3_core.c
+++ b/drivers/usb/mtu3/mtu3_core.c
@@ -237,7 +237,7 @@ void mtu3_ep_stall_set(struct mtu3_ep *m
 
 void mtu3_dev_on_off(struct mtu3 *mtu, int is_on)
 {
-	if (mtu->is_u3_ip && (mtu->max_speed == USB_SPEED_SUPER))
+	if (mtu->is_u3_ip && mtu->max_speed >= USB_SPEED_SUPER)
 		mtu3_ss_func_set(mtu, is_on);
 	else
 		mtu3_hs_softconn_set(mtu, is_on);
@@ -547,6 +547,9 @@ static void mtu3_set_speed(struct mtu3 *
 		mtu3_clrbits(mbase, U3D_USB3_CONFIG, USB3_EN);
 		/* HS/FS detected by HW */
 		mtu3_setbits(mbase, U3D_POWER_MANAGEMENT, HS_ENABLE);
+	} else if (mtu->max_speed == USB_SPEED_SUPER) {
+		mtu3_clrbits(mtu->ippc_base, SSUSB_U3_CTRL(0),
+			     SSUSB_U3_PORT_SSP_SPEED);
 	}
 
 	dev_info(mtu->dev, "max_speed: %s\n",
@@ -624,6 +627,10 @@ static irqreturn_t mtu3_link_isr(struct
 		udev_speed = USB_SPEED_SUPER;
 		maxpkt = 512;
 		break;
+	case MTU3_SPEED_SUPER_PLUS:
+		udev_speed = USB_SPEED_SUPER_PLUS;
+		maxpkt = 512;
+		break;
 	default:
 		udev_speed = USB_SPEED_UNKNOWN;
 		break;
@@ -825,14 +832,15 @@ int ssusb_gadget_init(struct ssusb_mtk *
 	case USB_SPEED_FULL:
 	case USB_SPEED_HIGH:
 	case USB_SPEED_SUPER:
+	case USB_SPEED_SUPER_PLUS:
 		break;
 	default:
 		dev_err(dev, "invalid max_speed: %s\n",
 			usb_speed_string(mtu->max_speed));
 		/* fall through */
 	case USB_SPEED_UNKNOWN:
-		/* default as SS */
-		mtu->max_speed = USB_SPEED_SUPER;
+		/* default as SSP */
+		mtu->max_speed = USB_SPEED_SUPER_PLUS;
 		break;
 	}
 
--- a/drivers/usb/mtu3/mtu3_gadget.c
+++ b/drivers/usb/mtu3/mtu3_gadget.c
@@ -89,6 +89,7 @@ static int mtu3_ep_enable(struct mtu3_ep
 
 	switch (mtu->g.speed) {
 	case USB_SPEED_SUPER:
+	case USB_SPEED_SUPER_PLUS:
 		if (usb_endpoint_xfer_int(desc) ||
 				usb_endpoint_xfer_isoc(desc)) {
 			interval = desc->bInterval;
@@ -456,7 +457,7 @@ static int mtu3_gadget_wakeup(struct usb
 		return  -EOPNOTSUPP;
 
 	spin_lock_irqsave(&mtu->lock, flags);
-	if (mtu->g.speed == USB_SPEED_SUPER) {
+	if (mtu->g.speed >= USB_SPEED_SUPER) {
 		mtu3_setbits(mtu->mac_base, U3D_LINK_POWER_CONTROL, UX_EXIT);
 	} else {
 		mtu3_setbits(mtu->mac_base, U3D_POWER_MANAGEMENT, RESUME);
--- a/drivers/usb/mtu3/mtu3_gadget_ep0.c
+++ b/drivers/usb/mtu3/mtu3_gadget_ep0.c
@@ -212,8 +212,8 @@ ep0_get_status(struct mtu3 *mtu, const s
 	case USB_RECIP_DEVICE:
 		result[0] = mtu->is_self_powered << USB_DEVICE_SELF_POWERED;
 		result[0] |= mtu->may_wakeup << USB_DEVICE_REMOTE_WAKEUP;
-		/* superspeed only */
-		if (mtu->g.speed == USB_SPEED_SUPER) {
+
+		if (mtu->g.speed >= USB_SPEED_SUPER) {
 			result[0] |= mtu->u1_enable << USB_DEV_STAT_U1_ENABLED;
 			result[0] |= mtu->u2_enable << USB_DEV_STAT_U2_ENABLED;
 		}
@@ -329,8 +329,8 @@ static int ep0_handle_feature_dev(struct
 		handled = handle_test_mode(mtu, setup);
 		break;
 	case USB_DEVICE_U1_ENABLE:
-		if (mtu->g.speed != USB_SPEED_SUPER ||
-			mtu->g.state != USB_STATE_CONFIGURED)
+		if (mtu->g.speed < USB_SPEED_SUPER ||
+		    mtu->g.state != USB_STATE_CONFIGURED)
 			break;
 
 		lpc = mtu3_readl(mbase, U3D_LINK_POWER_CONTROL);
@@ -344,8 +344,8 @@ static int ep0_handle_feature_dev(struct
 		handled = 1;
 		break;
 	case USB_DEVICE_U2_ENABLE:
-		if (mtu->g.speed != USB_SPEED_SUPER ||
-			mtu->g.state != USB_STATE_CONFIGURED)
+		if (mtu->g.speed < USB_SPEED_SUPER ||
+		    mtu->g.state != USB_STATE_CONFIGURED)
 			break;
 
 		lpc = mtu3_readl(mbase, U3D_LINK_POWER_CONTROL);
@@ -384,8 +384,8 @@ static int ep0_handle_feature(struct mtu
 		break;
 	case USB_RECIP_INTERFACE:
 		/* superspeed only */
-		if ((value == USB_INTRF_FUNC_SUSPEND)
-			&& (mtu->g.speed == USB_SPEED_SUPER)) {
+		if (value == USB_INTRF_FUNC_SUSPEND &&
+		    mtu->g.speed >= USB_SPEED_SUPER) {
 			/*
 			 * forward the request because function drivers
 			 * should handle it
--- a/drivers/usb/mtu3/mtu3_hw_regs.h
+++ b/drivers/usb/mtu3/mtu3_hw_regs.h
@@ -467,6 +467,7 @@
 #define SSUSB_VBUS_CHG_INT_B_EN		BIT(6)
 
 /* U3D_SSUSB_U3_CTRL_0P */
+#define SSUSB_U3_PORT_SSP_SPEED	BIT(9)
 #define SSUSB_U3_PORT_HOST_SEL		BIT(2)
 #define SSUSB_U3_PORT_PDN		BIT(1)
 #define SSUSB_U3_PORT_DIS		BIT(0)
