From eeef8a5da781e11746347b3cd9f1942be48ebaf0 Mon Sep 17 00:00:00 2001
From: Ian Molton <ian@mnementh.co.uk>
Date: Fri, 8 Dec 2017 13:10:30 +0100
Subject: [PATCH] brcmfmac: Tidy register definitions a little

Trivial tidy of register definitions.

Signed-off-by: Ian Molton <ian@mnementh.co.uk>
Acked-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 .../net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c |  4 ++--
 .../net/wireless/broadcom/brcm80211/brcmfmac/sdio.h   | 19 ++++++++++---------
 2 files changed, 12 insertions(+), 11 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c
@@ -153,9 +153,9 @@ int brcmf_sdiod_intr_register(struct brc
 		brcmf_sdiod_func0_wb(sdiodev, SDIO_CCCR_IENx, data, &ret);
 
 		/* redirect, configure and enable io for interrupt signal */
-		data = SDIO_SEPINT_MASK | SDIO_SEPINT_OE;
+		data = SDIO_CCCR_BRCM_SEPINT_MASK | SDIO_CCCR_BRCM_SEPINT_OE;
 		if (pdata->oob_irq_flags & IRQF_TRIGGER_HIGH)
-			data |= SDIO_SEPINT_ACT_HI;
+			data |= SDIO_CCCR_BRCM_SEPINT_ACT_HI;
 		brcmf_sdiod_func0_wb(sdiodev, SDIO_CCCR_BRCM_SEPINT,
 				     data, &ret);
 		sdio_release_host(sdiodev->func[1]);
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.h
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.h
@@ -52,16 +52,17 @@
 /* function 0 vendor specific CCCR registers */
 
 #define SDIO_CCCR_BRCM_CARDCAP			0xf0
-#define SDIO_CCCR_BRCM_CARDCAP_CMD14_SUPPORT	0x02
-#define SDIO_CCCR_BRCM_CARDCAP_CMD14_EXT	0x04
-#define SDIO_CCCR_BRCM_CARDCAP_CMD_NODEC	0x08
-#define SDIO_CCCR_BRCM_CARDCTRL		0xf1
-#define SDIO_CCCR_BRCM_CARDCTRL_WLANRESET	0x02
-#define SDIO_CCCR_BRCM_SEPINT			0xf2
+#define SDIO_CCCR_BRCM_CARDCAP_CMD14_SUPPORT	BIT(1)
+#define SDIO_CCCR_BRCM_CARDCAP_CMD14_EXT	BIT(2)
+#define SDIO_CCCR_BRCM_CARDCAP_CMD_NODEC	BIT(3)
+
+#define SDIO_CCCR_BRCM_CARDCTRL			0xf1
+#define SDIO_CCCR_BRCM_CARDCTRL_WLANRESET	BIT(1)
 
-#define  SDIO_SEPINT_MASK		0x01
-#define  SDIO_SEPINT_OE			0x02
-#define  SDIO_SEPINT_ACT_HI		0x04
+#define SDIO_CCCR_BRCM_SEPINT			0xf2
+#define SDIO_CCCR_BRCM_SEPINT_MASK		BIT(0)
+#define SDIO_CCCR_BRCM_SEPINT_OE		BIT(1)
+#define SDIO_CCCR_BRCM_SEPINT_ACT_HI		BIT(2)
 
 /* function 1 miscellaneous registers */
 
