/dts-v1/;

#include "mt7621.dtsi"

/ {
	compatible = "mediatek,ap-mt7621a-v60", "mediatek,mt7621-soc";
	model = "Mediatek AP-MT7621A-V60 EVB";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	sound {
		compatible = "simple-audio-card";
		simple-audio-card,name = "Audio-I2S";
		simple-audio-card,format = "i2s";
		simple-audio-card,bitclock-master = <&dailink0_master>;
		simple-audio-card,frame-master = <&dailink0_master>;
		simple-audio-card,widgets = 
			"Microphone", "Microphone Jack",
			"Headphone", "Headphone Jack";
		simple-audio-card,routing =
			"LINPUT1", "Microphone Jack",
			"RINPUT1", "Microphone Jack",
			"Headphone Jack", "HP_L",
			"Headphone Jack", "HP_R";
		simple-audio-card,mclk-fs = <256>;

		simple-audio-card,cpu {
			sound-dai = <&i2s>;
		};

		dailink0_master: simple-audio-card,codec {
			sound-dai = <&codec>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "uart2", "rgmii2";
			ralink,function = "gpio";
		};
	};
	i2s_pins: i2s {
		i2s {
			ralink,group = "uart3";
			ralink,function = "i2s";
		};
	};
};

&i2c {
	status = "okay";

	codec: wm8960@1a {
		#sound-dai-cells = <0>;
		compatible = "wlf,wm8960";
		reg = <0x1a>;
		wlf,shared-lrclk;
	};
};

&gdma {
	status = "okay";
};

&i2s {
	#sound-dai-cells = <0>;
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&i2s_pins>;
};

&spi0 {
	status = "okay";

	mx25l6405d@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "mx25l6405d","jedec,spi-nor";
		reg = <0 0>;
		spi-max-frequency = <10000000>;
		m25p,chunked-io = <32>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x30000>;
			read-only;
		};

		partition@30000 {
			label = "u-boot-env";
			reg = <0x30000 0x10000>;
			read-only;
		};

		factory: partition@40000 {
			label = "factory";
			reg = <0x40000 0x10000>;
			read-only;
		};

		partition@50000 {
			label = "firmware";
			reg = <0x50000 0x7b0000>;
		};
	};
};

&sdhci {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0x5>;
};

&pcie {
	status = "okay";
};
