From 561a7e69d2811f236266ff9222a1e683ebf8b9e0 Mon Sep 17 00:00:00 2001
From: Mathias Kresin <dev@kresin.me>
Date: Thu, 1 Mar 2018 20:50:29 +0100
Subject: [PATCH] ARM: dts: ipq4019: fix PCI range

The PCI range is invalid and PCI attached devices doen't work.

Signed-off-by: Mathias Kresin <dev@kresin.me>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -359,7 +359,7 @@
 			#size-cells = <2>;
 
 			ranges = <0x81000000 0 0x40200000 0x40200000 0 0x00100000
-				  0x82000000 0 0x48000000 0x48000000 0 0x10000000>;
+				  0x82000000 0 0x40300000 0x40300000 0 0x400000>;
 
 			interrupts = <GIC_SPI 141 IRQ_TYPE_NONE>;
 			interrupt-names = "msi";
