/dts-v1/;

#include "ar9.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "buffalo,wbmr-hp-g300h", "lantiq,xway", "lantiq,ar9";
	model = "Buffalo WBMR-HP-G300H";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;

		led-dsl = &dsl;
		led-internet = &online_green;
		led-usb = &usb;
		led-wifi = &wifi;
	};

	memory@0 {
		reg = <0x0 0x4000000>;
	};

	fpi@10000000 {
		localbus@0 {
			nor-boot@0 {
				compatible = "lantiq,nor";
				bank-width = <2>;
				reg = <0 0x0 0x2000000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partitions {
					compatible = "fixed-partitions";
					#address-cells = <1>;
					#size-cells = <1>;

					partition@0 {
						label = "uboot";
						reg = <0x00000 0x40000>;
						read-only;
					};

					partition@40000 {
						label = "uboot_env";
						reg = <0x40000 0x20000>;
						read-only;
					};

					partition@20000 {
						label = "firmware";
						reg = <0x60000 0x1f20000>;
					};

					boardconfig: partition@1fc0000 {
						label = "board";
						reg = <0x1fc0000 0x20000>;
						read-only;
					};

					partition@1fe0000 {
						label = "calibration";
						reg = <0x1fe0000 0x20000>;
						read-only;
					};
				};
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			state_default: pinmux {
				pci-in {
					lantiq,groups = "req1";
					lantiq,output = <0>;
					lantiq,open-drain = <1>;
					lantiq,pull = <2>;
				};
				pci-out {
					lantiq,groups = "gnt1";
					lantiq,output = <1>;
					lantiq,pull = <0>;
				};
				pci_rst {
					lantiq,pins = "io21";
					lantiq,pull = <0>;
					lantiq,output = <1>;
				};
			};
		};

		etop@E180000 {
			phy-mode = "rgmii";
			mtd-mac-address = <&boardconfig 0x10024>;
		};

		ifxhcd@E101000 {
			status = "okay";
			gpios = <&gpio 36 GPIO_ACTIVE_HIGH>;
		};

		pci@E105400 {
			status = "okay";
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		eject {
			label = "eject";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_EJECTCD>;
		};
		movie {
			label = "movie";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_VIDEO>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_green: power {
			label = "wbmr:green:power";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power2 {
			label = "wbmr:red:power";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		security {
			label = "wbmr:yellow:security";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "wbmr:green:wireless";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};
		dsl: dsl {
			label = "wbmr:green:dsl";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
		online_green: online {
			label = "wbmr:green:internet";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
		online2 {
			label = "wbmr:red:internet";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
		};
		movie {
			label = "wbmr:blue:movie";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};
		usb: usb {
			label = "wbmr:green:usb";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};
};
