From 179a445ae4ef36ec44f4aea18e5f42d21334d186 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Sat, 25 Feb 2017 12:39:25 +0100
Subject: [PATCH 4/6] bcm63xx_enet: use managed functions for clock/ioremap

Use managed functions where possible to reduce the amount of resource
handling on error and remove paths.

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 drivers/net/ethernet/broadcom/bcm63xx_enet.c | 54 +++++++---------------------
 1 file changed, 12 insertions(+), 42 deletions(-)

--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -1784,14 +1784,14 @@ static int bcm_enet_probe(struct platfor
 		clk_name = "enet1";
 	}
 
-	priv->mac_clk = clk_get(&pdev->dev, clk_name);
+	priv->mac_clk = devm_clk_get(&pdev->dev, clk_name);
 	if (IS_ERR(priv->mac_clk)) {
 		ret = PTR_ERR(priv->mac_clk);
 		goto out;
 	}
 	ret = clk_prepare_enable(priv->mac_clk);
 	if (ret)
-		goto out_put_clk_mac;
+		goto out;
 
 	/* initialize default and fetch platform data */
 	priv->rx_ring_size = BCMENET_DEF_RX_DESC;
@@ -1819,7 +1819,7 @@ static int bcm_enet_probe(struct platfor
 
 	if (priv->mac_id == 0 && priv->has_phy && !priv->use_external_mii) {
 		/* using internal PHY, enable clock */
-		priv->phy_clk = clk_get(&pdev->dev, "ephy");
+		priv->phy_clk = devm_clk_get(&pdev->dev, "ephy");
 		if (IS_ERR(priv->phy_clk)) {
 			ret = PTR_ERR(priv->phy_clk);
 			priv->phy_clk = NULL;
@@ -1827,7 +1827,7 @@ static int bcm_enet_probe(struct platfor
 		}
 		ret = clk_prepare_enable(priv->phy_clk);
 		if (ret)
-			goto out_put_clk_phy;
+			goto out_disable_clk_mac;
 	}
 
 	/* do minimal hardware init to be able to probe mii bus */
@@ -1921,14 +1921,8 @@ out_uninit_hw:
 	if (priv->phy_clk)
 		clk_disable_unprepare(priv->phy_clk);
 
-out_put_clk_phy:
-	if (priv->phy_clk)
-		clk_put(priv->phy_clk);
-
 out_disable_clk_mac:
 	clk_disable_unprepare(priv->mac_clk);
-out_put_clk_mac:
-	clk_put(priv->mac_clk);
 out:
 	free_netdev(dev);
 	return ret;
@@ -1964,12 +1958,10 @@ static int bcm_enet_remove(struct platfo
 	}
 
 	/* disable hw block clocks */
-	if (priv->phy_clk) {
+	if (priv->phy_clk)
 		clk_disable_unprepare(priv->phy_clk);
-		clk_put(priv->phy_clk);
-	}
+
 	clk_disable_unprepare(priv->mac_clk);
-	clk_put(priv->mac_clk);
 
 	free_netdev(dev);
 	return 0;
@@ -2752,26 +2744,20 @@ static int bcm_enetsw_probe(struct platf
 	if (ret)
 		goto out;
 
-	if (!request_mem_region(res_mem->start, resource_size(res_mem),
-				"bcm63xx_enetsw")) {
-		ret = -EBUSY;
+	priv->base = devm_ioremap_resource(&pdev->dev, res_mem);
+	if (IS_ERR(priv->base)) {
+		ret = PTR_ERR(priv->base);
 		goto out;
 	}
 
-	priv->base = ioremap(res_mem->start, resource_size(res_mem));
-	if (priv->base == NULL) {
-		ret = -ENOMEM;
-		goto out_release_mem;
-	}
-
-	priv->mac_clk = clk_get(&pdev->dev, "enetsw");
+	priv->mac_clk = devm_clk_get(&pdev->dev, "enetsw");
 	if (IS_ERR(priv->mac_clk)) {
 		ret = PTR_ERR(priv->mac_clk);
-		goto out_unmap;
+		goto out;
 	}
 	ret = clk_prepare_enable(priv->mac_clk);
 	if (ret)
-		goto out_put_clk;
+		goto out;
 
 	priv->rx_chan = 0;
 	priv->tx_chan = 1;
@@ -2803,15 +2789,6 @@ static int bcm_enetsw_probe(struct platf
 
 out_disable_clk:
 	clk_disable_unprepare(priv->mac_clk);
-
-out_put_clk:
-	clk_put(priv->mac_clk);
-
-out_unmap:
-	iounmap(priv->base);
-
-out_release_mem:
-	release_mem_region(res_mem->start, resource_size(res_mem));
 out:
 	free_netdev(dev);
 	return ret;
@@ -2823,20 +2800,13 @@ static int bcm_enetsw_remove(struct plat
 {
 	struct bcm_enet_priv *priv;
 	struct net_device *dev;
-	struct resource *res;
 
 	/* stop netdevice */
 	dev = platform_get_drvdata(pdev);
 	priv = netdev_priv(dev);
 	unregister_netdev(dev);
 
-	/* release device resources */
-	iounmap(priv->base);
-	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
-	release_mem_region(res->start, resource_size(res));
-
 	clk_disable_unprepare(priv->mac_clk);
-	clk_put(priv->mac_clk);
 
 	free_netdev(dev);
 	return 0;
