From 943b0832e0cf3afe5bd40ffb1885d06106122c5d Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Sun, 16 Jul 2017 12:49:49 +0200
Subject: [PATCH 1/4] bcm63xx_enet: just use "enet" as the clock name

Now that we have the individual clocks available as "enet" we
don't need to rely on the device id for them anymore.

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 drivers/net/ethernet/broadcom/bcm63xx_enet.c | 5 +----
 1 file changed, 1 insertion(+), 4 deletions(-)

--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -1736,7 +1736,6 @@ static int bcm_enet_probe(struct platfor
 	struct bcm63xx_enet_platform_data *pd;
 	struct resource *res_mem, *res_irq, *res_irq_rx, *res_irq_tx;
 	struct mii_bus *bus;
-	const char *clk_name;
 	int i, ret;
 
 	if (!bcm_enet_shared_base[0])
@@ -1777,14 +1776,12 @@ static int bcm_enet_probe(struct platfor
 	if (priv->mac_id == 0) {
 		priv->rx_chan = 0;
 		priv->tx_chan = 1;
-		clk_name = "enet0";
 	} else {
 		priv->rx_chan = 2;
 		priv->tx_chan = 3;
-		clk_name = "enet1";
 	}
 
-	priv->mac_clk = devm_clk_get(&pdev->dev, clk_name);
+	priv->mac_clk = devm_clk_get(&pdev->dev, "enet");
 	if (IS_ERR(priv->mac_clk)) {
 		ret = PTR_ERR(priv->mac_clk);
 		goto out;
