From 99c659cf345640fd0f733cbcaf4583cc2c868ec0 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 29 Apr 2013 13:21:48 +0200
Subject: [PATCH] rt2x00: rt2800lib: add RFCSR initialization for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800.h    |    1 +
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |  141 +++++++++++++++++++++++++++++++
 2 files changed, 142 insertions(+)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800.h
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800.h
@@ -2311,6 +2311,7 @@ struct mac_iveiv_entry {
 /*
  * RFCSR 2:
  */
+#define RFCSR2_RESCAL_BP		FIELD8(0x40)
 #define RFCSR2_RESCAL_EN		FIELD8(0x80)
 #define RFCSR2_RX2_EN_MT7620		FIELD8(0x02)
 #define RFCSR2_TX2_EN_MT7620		FIELD8(0x20)
--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -7707,6 +7707,144 @@ static void rt2800_init_rfcsr_5350(struc
 	rt2800_rfcsr_write(rt2x00dev, 63, 0x00);
 }
 
+static void rt2800_init_rfcsr_3883(struct rt2x00_dev *rt2x00dev)
+{
+	u8 rfcsr;
+
+	/* TODO: get the actual ECO value from the SoC */
+	const unsigned int eco = 5;
+
+	rt2800_rf_init_calibration(rt2x00dev, 2);
+
+	rt2800_rfcsr_write(rt2x00dev, 0, 0xe0);
+	rt2800_rfcsr_write(rt2x00dev, 1, 0x03);
+	rt2800_rfcsr_write(rt2x00dev, 2, 0x50);
+	rt2800_rfcsr_write(rt2x00dev, 3, 0x20);
+	rt2800_rfcsr_write(rt2x00dev, 4, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 5, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 6, 0x40);
+	rt2800_rfcsr_write(rt2x00dev, 7, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 8, 0x5b);
+	rt2800_rfcsr_write(rt2x00dev, 9, 0x08);
+	rt2800_rfcsr_write(rt2x00dev, 10, 0xd3);
+	rt2800_rfcsr_write(rt2x00dev, 11, 0x48);
+	rt2800_rfcsr_write(rt2x00dev, 12, 0x1a);
+	rt2800_rfcsr_write(rt2x00dev, 13, 0x12);
+	rt2800_rfcsr_write(rt2x00dev, 14, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 15, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 16, 0x00);
+
+	/* RFCSR 17 will be initialized later based on the
+	 * frequency offset stored in the EEPROM
+	 */
+
+	rt2800_rfcsr_write(rt2x00dev, 18, 0x40);
+	rt2800_rfcsr_write(rt2x00dev, 19, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 20, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 21, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 22, 0x20);
+	rt2800_rfcsr_write(rt2x00dev, 23, 0xc0);
+	rt2800_rfcsr_write(rt2x00dev, 24, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 25, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 26, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 27, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 28, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 29, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 30, 0x10);
+	rt2800_rfcsr_write(rt2x00dev, 31, 0x80);
+	rt2800_rfcsr_write(rt2x00dev, 32, 0x80);
+	rt2800_rfcsr_write(rt2x00dev, 33, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 34, 0x20);
+	rt2800_rfcsr_write(rt2x00dev, 35, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 36, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 37, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 38, 0x86);
+	rt2800_rfcsr_write(rt2x00dev, 39, 0x23);
+	rt2800_rfcsr_write(rt2x00dev, 40, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 41, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 42, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 43, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 44, 0x93);
+	rt2800_rfcsr_write(rt2x00dev, 45, 0xbb);
+	rt2800_rfcsr_write(rt2x00dev, 46, 0x60);
+	rt2800_rfcsr_write(rt2x00dev, 47, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 48, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 49, 0x8e);
+	rt2800_rfcsr_write(rt2x00dev, 50, 0x86);
+	rt2800_rfcsr_write(rt2x00dev, 51, 0x51);
+	rt2800_rfcsr_write(rt2x00dev, 52, 0x05);
+	rt2800_rfcsr_write(rt2x00dev, 53, 0x76);
+	rt2800_rfcsr_write(rt2x00dev, 54, 0x76);
+	rt2800_rfcsr_write(rt2x00dev, 55, 0x76);
+	rt2800_rfcsr_write(rt2x00dev, 56, 0xdb);
+	rt2800_rfcsr_write(rt2x00dev, 57, 0x3e);
+	rt2800_rfcsr_write(rt2x00dev, 58, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 59, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 60, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 61, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 62, 0x00);
+	rt2800_rfcsr_write(rt2x00dev, 63, 0x00);
+
+	/* TODO: rx filter calibration? */
+
+	rt2800_bbp_write(rt2x00dev, 137, 0x0f);
+
+	rt2800_bbp_write(rt2x00dev, 163, 0x9d);
+
+	rt2800_bbp_write(rt2x00dev, 105, 0x05);
+
+	rt2800_bbp_write(rt2x00dev, 179, 0x02);
+	rt2800_bbp_write(rt2x00dev, 180, 0x00);
+	rt2800_bbp_write(rt2x00dev, 182, 0x40);
+	rt2800_bbp_write(rt2x00dev, 180, 0x01);
+	rt2800_bbp_write(rt2x00dev, 182, 0x9c);
+
+	rt2800_bbp_write(rt2x00dev, 179, 0x00);
+
+	rt2800_bbp_write(rt2x00dev, 142, 0x04);
+	rt2800_bbp_write(rt2x00dev, 143, 0x3b);
+	rt2800_bbp_write(rt2x00dev, 142, 0x06);
+	rt2800_bbp_write(rt2x00dev, 143, 0xa0);
+	rt2800_bbp_write(rt2x00dev, 142, 0x07);
+	rt2800_bbp_write(rt2x00dev, 143, 0xa1);
+	rt2800_bbp_write(rt2x00dev, 142, 0x08);
+	rt2800_bbp_write(rt2x00dev, 143, 0xa2);
+	rt2800_bbp_write(rt2x00dev, 148, 0xc8);
+
+	if (eco == 5) {
+		rt2800_rfcsr_write(rt2x00dev, 32, 0xd8);
+		rt2800_rfcsr_write(rt2x00dev, 33, 0x32);
+	}
+
+	rfcsr = rt2800_rfcsr_read(rt2x00dev, 2);
+	rt2x00_set_field8(&rfcsr, RFCSR2_RESCAL_BP, 0);
+	rt2x00_set_field8(&rfcsr, RFCSR2_RESCAL_EN, 1);
+	rt2800_rfcsr_write(rt2x00dev, 2, rfcsr);
+	msleep(1);
+	rt2x00_set_field8(&rfcsr, RFCSR2_RESCAL_EN, 0);
+	rt2800_rfcsr_write(rt2x00dev, 2, rfcsr);
+
+	rfcsr = rt2800_rfcsr_read(rt2x00dev, 1);
+	rt2x00_set_field8(&rfcsr, RFCSR1_RF_BLOCK_EN, 1);
+	rt2800_rfcsr_write(rt2x00dev, 1, rfcsr);
+
+	rfcsr = rt2800_rfcsr_read(rt2x00dev, 6);
+	rfcsr |= 0xc0;
+	rt2800_rfcsr_write(rt2x00dev, 6, rfcsr);
+
+	rfcsr = rt2800_rfcsr_read(rt2x00dev, 22);
+	rfcsr |= 0x20;
+	rt2800_rfcsr_write(rt2x00dev, 22, rfcsr);
+
+	rfcsr = rt2800_rfcsr_read(rt2x00dev, 46);
+	rfcsr |= 0x20;
+	rt2800_rfcsr_write(rt2x00dev, 46, rfcsr);
+
+	rfcsr = rt2800_rfcsr_read(rt2x00dev, 20);
+	rfcsr &= ~0xee;
+	rt2800_rfcsr_write(rt2x00dev, 20, rfcsr);
+}
+
 static void rt2800_init_rfcsr_5390(struct rt2x00_dev *rt2x00dev)
 {
 	rt2800_rf_init_calibration(rt2x00dev, 2);
@@ -8549,6 +8687,9 @@ static void rt2800_init_rfcsr(struct rt2
 	case RT3390:
 		rt2800_init_rfcsr_3390(rt2x00dev);
 		break;
+	case RT3883:
+		rt2800_init_rfcsr_3883(rt2x00dev);
+		break;
 	case RT3572:
 		rt2800_init_rfcsr_3572(rt2x00dev);
 		break;
