From: Felix Fietkau <nbd@nbd.name>
Date: Tue, 13 Nov 2018 20:29:03 +0100
Subject: [PATCH] mac80211: ignore tx status for PS stations in
 ieee80211_tx_status_ext

Make it behave like regular ieee80211_tx_status calls, except for the lack of
filtered frame processing.
This fixes spurious low-ack triggered disconnections with powersave clients
connected to an AP.

Fixes: f027c2aca0cf4 ("mac80211: add ieee80211_tx_status_noskb")
Cc: stable@vger.kernel.org
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/mac80211/status.c
+++ b/net/mac80211/status.c
@@ -976,6 +976,8 @@ void ieee80211_tx_status_ext(struct ieee
 			/* Track when last TDLS packet was ACKed */
 			if (test_sta_flag(sta, WLAN_STA_TDLS_PEER_AUTH))
 				sta->status_stats.last_tdls_pkt_time = jiffies;
+		} else if (test_sta_flag(sta, WLAN_STA_PS_STA)) {
+			return;
 		} else {
 			ieee80211_lost_packet(sta, info);
 		}
