/dts-v1/;

#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv7525pw", "lantiq,xway", "lantiq,danube";
	model = "Speedport W303V Typ A";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;

		led-dsl = &power_green;
		led-internet = &online;
		led-wifi = &wifi;
	};

	memory@0 {
		reg = <0x0 0x2000000>;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 29 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";
		power_green: power {
			label = "arv7525pw:green:power";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power1 {
			label = "arv7525pw:red:power";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		online: online {
			label = "arv7525pw:green:online";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		voice {
			label = "arv7525pw:green:telefonie";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		voice2 {
			label = "arv7525pw:red:telefonie";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "arv7525pw:green:wlan";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		exin {
			lantiq,groups = "exin1";
			lantiq,function = "exin";
		};
		pci {
			lantiq,groups = "gnt1", "req1";
			lantiq,function = "pci";
		};
	};
};

&gsw {
	phy-mode = "mii";
	mtd-mac-address = <&boardconfig 0x16>;
};

&localbus {
	nor@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x2000000>;
		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x10000>;
				read-only;
			};

			partition@10000 {
				label = "uboot_env";
				reg = <0x10000 0x10000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0x3d0000>;
			};

			boardconfig: partition@400000 {
				label = "board_config";
				reg = <0x3f0000 0x10000>;
				read-only;
			};
		};
	};
};

&pci0 {
	status = "okay";
	interrupt-map = <0x7000 0 0 1 &icu0 135 1>;

	wifi@0,0 {
		compatible = "pci0,0";
		reg = <0x7000 0 0 0 0>;
		ralink,mtd-eeprom = <&boardconfig 0x410>;
	};
};

&vmmc {
	status = "okay";
	gpios = <&gpio 31 GPIO_ACTIVE_HIGH>;
};
