From 1567cde49a0f2304e18c08e2ccd830e0686fc0a7 Mon Sep 17 00:00:00 2001
From: Sean Wang <sean.wang@mediatek.com>
Date: Wed, 18 Oct 2017 16:28:42 +0800
Subject: [PATCH 116/224] dt-bindings: arm: mediatek: add MT7622 string to the
 PMIC wrapper doc

Signed-off-by: Chenglin Xu <chenglin.xu@mediatek.com>
Signed-off-by: Sean Wang <sean.wang@mediatek.com>
Acked-by: Rob Herring <robh@kernel.org>
Signed-off-by: Matthias Brugger <matthias.bgg@gmail.com>
---
 Documentation/devicetree/bindings/soc/mediatek/pwrap.txt | 6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

--- a/Documentation/devicetree/bindings/soc/mediatek/pwrap.txt
+++ b/Documentation/devicetree/bindings/soc/mediatek/pwrap.txt
@@ -19,6 +19,7 @@ IP Pairing
 Required properties in pwrap device node.
 - compatible:
 	"mediatek,mt2701-pwrap" for MT2701/7623 SoCs
+	"mediatek,mt7622-pwrap" for MT7622 SoCs
 	"mediatek,mt8135-pwrap" for MT8135 SoCs
 	"mediatek,mt8173-pwrap" for MT8173 SoCs
 - interrupts: IRQ for pwrap in SOC
@@ -36,9 +37,12 @@ Required properties in pwrap device node
 - clocks: Must contain an entry for each entry in clock-names.
 
 Optional properities:
-- pmic: Mediatek PMIC MFD is the child device of pwrap
+- pmic: Using either MediaTek PMIC MFD as the child device of pwrap
   See the following for child node definitions:
   Documentation/devicetree/bindings/mfd/mt6397.txt
+  or the regulator-only device as the child device of pwrap, such as MT6380.
+  See the following definitions for such kinds of devices.
+  Documentation/devicetree/bindings/regulator/mt6380-regulator.txt
 
 Example:
 	pwrap: pwrap@1000f000 {
