From 0e1a71d84585ec33b479c2cb8c8d65a4f6734dbe Mon Sep 17 00:00:00 2001
From: Thomas Richard <thomas.richard@bootlin.com>
Date: Wed, 4 Dec 2024 14:26:52 +0100
Subject: [PATCH] Revert "feat(stm32mp1-fdts): remove RTC clock configuration"

This reverts commit 703a581e2522bffe21b421c98994dc02aed2934c.
---
 fdts/stm32mp135f-dk.dts   | 2 ++
 fdts/stm32mp157c-ed1.dts  | 2 ++
 fdts/stm32mp15xx-dkx.dtsi | 2 ++
 3 files changed, 6 insertions(+)

--- a/fdts/stm32mp135f-dk.dts
+++ b/fdts/stm32mp135f-dk.dts
@@ -190,6 +190,7 @@
 		CLK_AXI_PLL2P
 		CLK_MLAHBS_PLL3
 		CLK_CKPER_HSE
+		CLK_RTC_LSE
 		CLK_SDMMC1_PLL4P
 		CLK_SDMMC2_PLL4P
 		CLK_STGEN_HSE
@@ -211,6 +212,7 @@
 		DIV(DIV_APB4, 1)
 		DIV(DIV_APB5, 2)
 		DIV(DIV_APB6, 1)
+		DIV(DIV_RTC, 0)
 	>;
 
 	st,pll_vco {
--- a/fdts/stm32mp157c-ed1.dts
+++ b/fdts/stm32mp157c-ed1.dts
@@ -194,6 +194,7 @@
 		CLK_MPU_PLL1P
 		CLK_AXI_PLL2P
 		CLK_MCU_PLL3P
+		CLK_RTC_LSE
 		CLK_MCO1_DISABLED
 		CLK_MCO2_DISABLED
 		CLK_CKPER_HSE
@@ -242,6 +243,7 @@
 		DIV(DIV_APB3, 1)
 		DIV(DIV_APB4, 1)
 		DIV(DIV_APB5, 2)
+		DIV(DIV_RTC, 23)
 		DIV(DIV_MCO1, 0)
 		DIV(DIV_MCO2, 0)
 	>;
--- a/fdts/stm32mp15xx-dkx.dtsi
+++ b/fdts/stm32mp15xx-dkx.dtsi
@@ -198,6 +198,7 @@
 		CLK_MPU_PLL1P
 		CLK_AXI_PLL2P
 		CLK_MCU_PLL3P
+		CLK_RTC_LSE
 		CLK_MCO1_DISABLED
 		CLK_MCO2_DISABLED
 		CLK_CKPER_HSE
@@ -246,6 +247,7 @@
 		DIV(DIV_APB3, 1)
 		DIV(DIV_APB4, 1)
 		DIV(DIV_APB5, 2)
+		DIV(DIV_RTC, 23)
 		DIV(DIV_MCO1, 0)
 		DIV(DIV_MCO2, 0)
 	>;
