From 97df847f8f895cc2692bb0e4e933269c275da378 Mon Sep 17 00:00:00 2001
From: Weijie Gao <weijie.gao@mediatek.com>
Date: Tue, 2 Mar 2021 15:47:45 +0800
Subject: [PATCH 35/71] board: mediatek: add more network configurations

Make the network configurations uniform for mediatek boards

Signed-off-by: Weijie Gao <weijie.gao@mediatek.com>
---
 include/configs/mt7622.h | 3 ++-
 include/configs/mt7623.h | 1 +
 include/configs/mt7629.h | 1 +
 include/configs/mt7981.h | 5 +++++
 include/configs/mt7986.h | 5 +++++
 5 files changed, 14 insertions(+), 1 deletion(-)

--- a/include/configs/mt7622.h
+++ b/include/configs/mt7622.h
@@ -19,6 +19,7 @@
 
 /* Ethernet */
 #define CONFIG_IPADDR			192.168.1.1
-#define CONFIG_SERVERIP			192.168.1.3
+#define CONFIG_SERVERIP			192.168.1.2
+#define CONFIG_NETMASK			255.255.255.0
 
 #endif
--- a/include/configs/mt7623.h
+++ b/include/configs/mt7623.h
@@ -35,6 +35,7 @@
 /* Ethernet */
 #define CONFIG_IPADDR			192.168.1.1
 #define CONFIG_SERVERIP			192.168.1.2
+#define CONFIG_NETMASK			255.255.255.0
 
 #ifdef CONFIG_DISTRO_DEFAULTS
 
--- a/include/configs/mt7629.h
+++ b/include/configs/mt7629.h
@@ -30,5 +30,6 @@
 /* Ethernet */
 #define CONFIG_IPADDR			192.168.1.1
 #define CONFIG_SERVERIP			192.168.1.2
+#define CONFIG_NETMASK			255.255.255.0
 
 #endif
--- a/include/configs/mt7981.h
+++ b/include/configs/mt7981.h
@@ -18,4 +18,9 @@
 /* DRAM */
 #define CONFIG_SYS_SDRAM_BASE		0x40000000
 
+/* Ethernet */
+#define CONFIG_IPADDR			192.168.1.1
+#define CONFIG_SERVERIP			192.168.1.2
+#define CONFIG_NETMASK			255.255.255.0
+
 #endif
--- a/include/configs/mt7986.h
+++ b/include/configs/mt7986.h
@@ -18,4 +18,9 @@
 /* DRAM */
 #define CONFIG_SYS_SDRAM_BASE		0x40000000
 
+/* Ethernet */
+#define CONFIG_IPADDR			192.168.1.1
+#define CONFIG_SERVERIP			192.168.1.2
+#define CONFIG_NETMASK			255.255.255.0
+
 #endif
