From b5beecb580376cd8d959eb990abece6a748a3ce3 Mon Sep 17 00:00:00 2001
From: Corentin Labbe <clabbe.montjoie@gmail.com>
Date: Tue, 24 Oct 2017 19:57:12 +0200
Subject: [PATCH] net: stmmac: snps, dwmac-mdio MDIOs are automatically
 registered

stmmac bindings docs said that its mdio node must have
compatible = "snps,dwmac-mdio";
Since dwmac-sun8i does not have any good reasons to not doing it, all
their MDIO node must have it.

Since these compatible is automatically registered, dwmac-sun8i compatible
does not need to be in need_mdio_ids.

Signed-off-by: Corentin Labbe <clabbe.montjoie@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/stmicro/stmmac/stmmac_platform.c | 4 ----
 1 file changed, 4 deletions(-)

--- a/drivers/net/ethernet/stmicro/stmmac/stmmac_platform.c
+++ b/drivers/net/ethernet/stmicro/stmmac/stmmac_platform.c
@@ -318,10 +318,6 @@ static int stmmac_dt_phy(struct plat_stm
 	bool mdio = true;
 	static const struct of_device_id need_mdio_ids[] = {
 		{ .compatible = "snps,dwc-qos-ethernet-4.10" },
-		{ .compatible = "allwinner,sun8i-a83t-emac" },
-		{ .compatible = "allwinner,sun8i-h3-emac" },
-		{ .compatible = "allwinner,sun8i-v3s-emac" },
-		{ .compatible = "allwinner,sun50i-a64-emac" },
 		{},
 	};
 
