From c61ef9c4707e38edeafad1bd4d01080d0e0a10da Mon Sep 17 00:00:00 2001
From: Sean Wang <sean.wang@mediatek.com>
Date: Wed, 17 Jan 2018 00:52:27 +0800
Subject: [PATCH 222/224] arm64: dts: mt7622: add High-Speed DMA device nodes

add High-Speed DMA (HSDMA) nodes

Signed-off-by: Sean Wang <sean.wang@mediatek.com>
---
 arch/arm64/boot/dts/mediatek/mt7622.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/arch/arm64/boot/dts/mediatek/mt7622.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7622.dtsi
@@ -715,6 +715,16 @@
 		#reset-cells = <1>;
 	};
 
+	hsdma: dma-controller@1b007000 {
+		compatible = "mediatek,mt7622-hsdma";
+		reg = <0 0x1b007000 0 0x1000>;
+		interrupts = <GIC_SPI 219 IRQ_TYPE_LEVEL_LOW>;
+		clocks = <&ethsys CLK_ETH_HSDMA_EN>;
+		clock-names = "hsdma";
+		power-domains = <&scpsys MT7622_POWER_DOMAIN_ETHSYS>;
+		#dma-cells = <1>;
+	};
+
 	eth: ethernet@1b100000 {
 		compatible = "mediatek,mt7622-eth",
 			     "mediatek,mt2701-eth",
