From: Vijay Viswanath <vviswana@codeaurora.org>
Date: Wed, 27 Sep 2017 11:04:42 +0530
Subject: [PATCH v2 3/4] mmc: Kconfig: Enable CONFIG_MMC_SDHCI_IO_ACCESSORS

Enable CONFIG_MMC_SDHCI_IO_ACCESSORS so that SDHC controller specific
register read and write APIs, if registered, can be used.

Signed-off-by: Vijay Viswanath <vviswana@codeaurora.org>
Acked-by: Adrian Hunter <adrian.hunter@intel.com>
---
 drivers/mmc/host/Kconfig | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mmc/host/Kconfig
+++ b/drivers/mmc/host/Kconfig
@@ -420,6 +420,7 @@ config MMC_SDHCI_MSM
 	tristate "Qualcomm SDHCI Controller Support"
 	depends on ARCH_QCOM || (ARM && COMPILE_TEST)
 	depends on MMC_SDHCI_PLTFM
+	select MMC_SDHCI_IO_ACCESSORS
 	help
 	  This selects the Secure Digital Host Controller Interface (SDHCI)
 	  support present in Qualcomm SOCs. The controller supports
